Test Environment Paper (L1)

1. What do not need to do when setup test environment for ‘ea-carp-urp1’ (Single Choice)
2. Add phone number on macro.properties
3. Config USBRelay ID on Webconsole
4. Add the order of podcast to macro.propertes
5. Add phone number on Webconsole
6. Add carp1-normal=Relay1 on macro.propertes
7. What do not need to do when setup test environment for VR (Single Choice)
8. Uncheck the ‘AGC’ on Microphone properties
9. Turn off the ‘TCP’ on bench
10. Do insulation on AUX cable
11. Unplug the AUX cable from sound card when tester leave for a long time
12. What need to do when execute MY21GB Onstar cases automatically on bench (Multiple Choice)
13. Turn off the ‘TCP’ on bench
14. Set IP address which for Node connect with CSM to 192.168.1.102
15. Modify ‘PLATFORM = globalB’ on ecud.cfg
16. Turn off the VBI on Webconsole
17. Open the ECUD on Webconsole
18. What you don’t need to do when setup test environment for ‘ea-bt1c1-normal’ (Single Choice)
19. Config phone number on Webconsole – DUT Under Device – Phone Number1
20. Config phone number on Webconsole -- Companion Device(s) -- Phone Number 1
21. The ‘Stay awake’ button is open on phone side
22. Config the phone’s ID on Webconsole – DUT Under Device -- Device ID
23. Select the index ‘1’ on Webconsole -- Companion Device(s)
24. Which action is wrong when turn off the MY21GB or MY22 bench (Single Choice)
25. Send the Park message, press the Engine button, press the door button and wait for sleep, then turn off the main power switch of bench
26. Turn the CSM Switch on the bench panel to off side, then turn off the main power switch of bench
27. What is not the reason if the NODE on TMS is offline (Single Choice)
28. The CSM’s name is different between Webconsole and TMS
29. The companion phone’s name is different between Webconsole and TMS
30. The Android auto’s id is difference between Webconsole and TMS
31. The Node ID is difference between Webconsole and TMS
32. What do not need to do when setup test environment for MY22 ignition Automation test (Single Choice)
33. CAN tool need connect with CSM port
34. CAN tool need connect with BCM port
35. CAN tool need connect with CGM port
36. Config UABRelay ID on Webconsole
37. Config the ext\_functions file
38. Which action is wrong for MY21 Navigation feature setup (Single Choice)
39. Change the navigation to day mode
40. Unplug the SD card when the CSM is power up
41. The navigation should locate on land
42. Unplug the SD card when the CSM is power off
43. Which is wrong when setup Android auto (Single Choice)
44. Double check the Bluetooth name if it is right
45. Launch the Android auto under each user if the CSM config as local user
46. It displays as ‘Android auto’ under the ‘Phone’
47. It displays as ‘Android auto – Outgoing and Incoming Calls’
48. What action is wrong before execute case on TMS (Single Choice)
49. Check the NODEs and DUT are online on TMS
50. Start the VBI in Webconsole
51. Do the ‘Environment Check’ on Webconsole
52. Turn on the ‘Windows Defender Firewall’ on
53. Config the debugboard 3rd port on Webconsol